目录

[1. 修改记录 2](#_Toc75763328)

[2. 用户登录 4](#_Toc75763329)

[3. 用户登出 4](#_Toc75763330)

[4. 超脑设备添加 5](#_Toc75763331)

[5. 超脑设备删除 6](#_Toc75763332)

[6. 超脑列表信息获取 7](#_Toc75763333)

[7. 超脑设备信息设置 8](#_Toc75763334)

[8. 摄像头设备信息设置 10](#_Toc75763335)

[9. 告警级别获取 11](#_Toc75763336)

[10. 告警级别设置 12](#_Toc75763337)

[11. 智能告警数据请求 12](#_Toc75763338)

[12. 告警占比数据获取 14](#_Toc75763339)

[13. 告警数据时段分析 15](#_Toc75763340)

[14. 实时车俩数据统计推送 19](#_Toc75763341)

[15. 拐入率车辆列表获取 19](#_Toc75763342)

[16. 拐入率数据推送 20](#_Toc75763343)

[17. 告警推送 20](#_Toc75763344)

[18. 临街车辆数据获取 20](#_Toc75763345)

[19. 进站率数据请求 21](#_Toc75763346)

[20. 站内车辆数据请求 22](#_Toc75763347)

[21. 车辆历史记录数据请求 26](#_Toc75763348)

[22. 站内加油趋势数据请求 27](#_Toc75763349)

[23. 站内车牌区域分析请求 28](#_Toc75763350)

[24. 站内单台车辆加油趋势分析请求 29](#_Toc75763351)

[25. 站内加油（汽油，柴油）车辆数量分析 29](#_Toc75763352)

[26. 出站车辆数据分析 30](#_Toc75763353)

[27. 停留时间占比分析 35](#_Toc75763354)

[28. 加油效率分析 35](#_Toc75763355)

[29. 车辆轨迹数据请求 39](#_Toc75763356)

[30. 获取考勤打卡记录 41](#_Toc75763357)

[31. 推送考勤打卡 43](#_Toc75763358)

[32. 推送顾客进店次数 44](#_Toc75763359)

[33. 推送客流量 44](#_Toc75763360)

[34. 获取当日打卡人员考勤数据 45](#_Toc75763361)

[35. 获取当日所有顾客进店数据 46](#_Toc75763362)

## 修改记录

|  |  |  |
| --- | --- | --- |
| 版本 | 修改人 | 备注 |
| V1.0.0 | 赵叶波 | 起草协议 |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

## 用户登录

用户登录请求

Topic: station/mainserver/pullmsg

|  |  |  |
| --- | --- | --- |
| 参数定义 | 参数说明 | 取值范围 |
| username | 用户名 | 字符串，长度<128 |
| password | 密码 | 字符串，长度<128 |
| clitopic | mainserver/随机数/pullmsg | 字符串，长度<128 |
| {     "cmd":"loginmainserver",     "method":"request",     "msgid":"0123456",     "data":{         "username":"gzadmin@u",         "password":"gzadmin@p"     } } | | |

用户登录回复：

Topic: mainserver/username\_包名\_UDID\_当前毫秒数/pullmsg

|  |  |  |
| --- | --- | --- |
| 参数定义 | 参数说明 | 取值范围 |
| sessionid | 用户ID（后续对用户操作需要带此ID） | 字符串，长度<128 |
| **{**  "cmd"**:** "loginmainserver"**,**  "data"**:** **{**  "sessionid"**:** "65536"**,**  "userid"**:** "12585"  **},**  "method"**:** "response"**,**  "msgid"**:** "0123456"**,**  "statuscode"**:** 200**/**401  **}** | | |

## 用户登出

用户登出请求

Topic:app/mainserver/pullmsg

|  |  |  |
| --- | --- | --- |
| 参数定义 | 参数说明 | 取值范围 |
| username | 用户名 | 字符串，长度<128 |
| password | 密码 | 字符串，长度<128 |
| sessionid | 用户登录成功返回的ID | 字符串，长度<128 |
| {  "cmd" : "loginoutmainserver",  "method":"request",  "msgid":"0123456",  "sessionid" : "65536"  } | | |

用户登出回复

Topic:mainserver/username\_包名\_UDID\_当前秒数/pullmsg

|  |  |  |
| --- | --- | --- |
| 参数定义 | 参数说明 | 取值范围 |
| statuscode | 状态码 | 200/401/500(Http状态码) |
| {  "cmd" : "loginoutmainserver",  "method":"response",  "msgid":"0123456",  "statuscode" : 200  } | | |

## 超脑设备添加

超脑设备添加请求

Topic:app/mainserver/pullmsg

|  |  |  |
| --- | --- | --- |
| 参数定义 | 参数说明 | 取值范围 |
| dvrname | 设备名称 | 字符串，长度<64 |
| username | 用户名 | 字符串，长度<128 |
| password | 密码 | 字符串，长度<128 |
| ipadress | 超脑设备ip地址 | 字符串，长度<128 |
| Port | 端口号 | INT |
| **{**  "cmd"**:** "sdkdeviceadd"**,**  "method"**:** "response"**,**  "msgid"**:** "0123456"**,**  "sessionid"**:** "65536"**,**  "data"**:** **{**  "dvrname"**:** "shshas"**,**  "username"**:** "admin"**,**  "password"**:** "125854"**,**  "ipadress"**:** "192.168.0.104"**,**  "port": 8000  }  **}** | | |
|  | | |

超脑设备添加回复

Topic:mainserver/username\_包名\_UDID\_当前秒数/pullmsg

|  |  |  |
| --- | --- | --- |
| 参数定义 | 参数说明 | 取值范围 |
| statuscode | 状态码 | 200/401/500(Http状态码) |
| {  "cmd" : "sdkdeviceadd",  "method":"response",  "msgid":"0123456",  "statuscode" : 200  } | | |

## 超脑设备删除

超脑设备删除请求

Topic:app/mainserver/pullmsg

|  |  |  |
| --- | --- | --- |
| 参数定义 | 参数说明 | 取值范围 |
| sdvrserialnumber | 超脑序列号 | 字符串，长度<128 |
| **{**  "cmd"**:** "sdkdevicedel"**,**  "method"**:** "response"**,**  "msgid"**:** "0123456"**,**  "sessionid"**:** "65536"**,**  "data"**:** **{**  "sdvrserialnumber"**:** "iDS-9608NX-I8/FA0820210111CCRRF40231916WCVU"**,**  }  **}** | | |

超脑设备删除回复

Topic:mainserver/username\_包名\_UDID\_当前秒数/pullmsg

|  |  |  |
| --- | --- | --- |
| 参数定义 | 参数说明 | 取值范围 |
| statuscode | 状态码 | 200/401/500(Http状态码) |
| {  "cmd" : "sdkdevicedel",  "method":"response",  "msgid":"0123456",  "statuscode" : 200  } | | |

## 超脑列表信息获取

超脑列表信息获取请求

Topic:app/mainserver/pullmsg

|  |  |  |
| --- | --- | --- |
| 参数定义 | 参数说明 | 取值范围 |
| **{**  "cmd"**:** "sdkdevicelistget"**,**  "method"**:** "response"**,**  "msgid"**:** "0123456"**,**  "sessionid"**:** "65536"**,**  **}** | | |

超脑列表信息获取请求回复

Topic:mainserver/username\_包名\_UDID\_当前秒数/pullmsg

|  |  |  |
| --- | --- | --- |
| 参数定义 | 参数说明 | 取值范围 |
| statuscode | 状态码 | 200/401/500(Http状态码) |
| {     "cmd":"sdkdevicelistget",     "method":"response",     "msgid":"0123456",     "data":{         "Dvrlist":[             {                 "port":8000,                 "channels":64,                 "Dvrname":"",                 "IPaddress":"10.67.0.62",                 "username":"admin",                 "password":"gaozhi2014",                 "serialnumber":"iDS-9664NX-I8/X1620200922CCRRE85972695WCVU",                 "IPClist":[                     {                         "online":1,                         "channel":0,                         "devicetype":2,                         "devicename":"chn\_1",                         "deviceIP":"10.67.0.100"                     },                     {                         "online":1,                         "channel":1,                         "devicetype":2,                         "devicename":"chn\_2",                         "deviceIP":"10.67.0.100"                     },                     {                         "online":1,                         "channel":2,                         "devicetype":1,                         "devicename":"chn\_3",                         "deviceIP":"10.67.0.123"                     },                     {                         "online":1,                         "channel":3,                         "devicetype":1,                         "devicename":"chn\_4",                         "deviceIP":"10.67.0.124"                     }                 ]             }         ]     },     "statuscode":200 } | | |

## 超脑设备信息设置

超脑设备信息设置请求

Topic:app/mainserver/pullmsg

|  |  |  |
| --- | --- | --- |
| 参数定义 | 参数说明 | 取值范围 |
| sdvrserialnumber | 超脑序列号 | 字符串，长度<128 |
| dvrname | 超脑名称 | 字符串，长度<128 |
| ipcamname | 摄像头名称 | 字符串，长度<128 |
| Devicetype | 设备类型 | INT |
| {     "cmd":"sdkdevicelistget",     "method":"response",     "msgid":"0123456",     "data":{         "Dvrlist":[             {                 "port":8000,                 "channels":64,                 "Dvrname":"超脑1",                 "IPaddress":"10.67.0.62",                 "username":"admin",                 "password":"gaozhi2014",                 "serialnumber":"iDS-9664NX-I8/X1620200922CCRRE85972695WCVU",                 "IPClist":[                     {                         "online":1,                         "channel":0,                         "devicetype":2,                         "devicename":"临街\_1",                         "deviceIP":"10.67.0.100"                     },                     {                         "online":1,                         "channel":1,                         "devicetype":2,                         "devicename":"临街\_2",                         "deviceIP":"10.67.0.100"                     },                     {                         "online":1,                         "channel":2,                         "devicetype":2,                         "devicename":"临街\_3",                         "deviceIP":"10.67.0.123"                     },                     {                         "online":1,                         "channel":3,                         "devicetype":2,                         "devicename":"临街\_4",                         "deviceIP":"10.67.0.124"                     }                 ]             }         ]     },     "statuscode":200 } | | |

超脑设备信息设置回复

Topic:mainserver/username\_包名\_UDID\_当前秒数/pullmsg

|  |  |  |
| --- | --- | --- |
| 参数定义 | 参数说明 | 取值范围 |
| statuscode | 状态码 | 200/401/500(Http状态码) |
| {  "cmd" : "sdkdevicedel",  "method":"response",  "msgid":"0123456",  "statuscode" : 200  } | | |

## 摄像头设备信息设置

摄像头设备信息设置请求

Topic:app/mainserver/pullmsg

|  |  |  |
| --- | --- | --- |
| 参数定义 | 参数说明 | 取值范围 |
| channel | 通道号 | INT |
| devicetype | 设备类型 | INT |
| devicename | 摄像头名称 | 字符串，长度<64 |
| serialnumber | 超脑序列号 | 字符串，长度<64 |
| {  "clitopic": "CCSMP/62356210444/pullmsg",  "cmd": "sdkdeviceipcamset",  "method": "request",  "msgid": "0123456",  "sessionid": "262176",  "data": {  "channel": 2,  "devicetype": 1,  "devicename": "临街\_1",  "serialnumber": "iDS-9664NX-I8/X1620200922CCRRE85972695WCVU",  }  } | | |

超脑设备信息设置回复

Topic:mainserver/username\_包名\_UDID\_当前秒数/pullmsg

|  |  |  |
| --- | --- | --- |
| 参数定义 | 参数说明 | 取值范围 |
| statuscode | 状态码 | 200/401/500(Http状态码) |
| {  "cmd" : " sdkdeviceipcamset ",  "method":"response",  "msgid":"0123456",  "statuscode" : 200  } | | |

## 告警级别获取

告警级别获取请求

Topic:app/mainserver/pullmsg

|  |  |  |
| --- | --- | --- |
| 参数定义 | 参数说明 | 取值范围 |
| {  "cmd": " sdkdevicealarmget",  "method": "request",  "msgid": "0123456",  "sessionid": "262176",  } | | |

告警级别获取回复

Topic:mainserver/username\_包名\_UDID\_当前秒数/pullmsg

|  |  |  |
| --- | --- | --- |
| 参数定义 | 参数说明 | 取值范围 |
| smoke | 烟雾告警 | INT |
| hightemp | 高温告警 | INT |
| statuscode | 状态码 | 200/401/500(Http状态码) |
| {  "cmd" : "sdkdevicealarmget ",  "method":"response",  "msgid":"0123456",  "data": {  "smoke": 1,  "hightemp": 1,  }  "statuscode" : 200  } | | |

## 告警级别设置

告警级别设置请求

Topic:app/mainserver/pullmsg

|  |  |  |
| --- | --- | --- |
| 参数定义 | 参数说明 | 取值范围 |
| smoke | 烟雾告警 | INT |
| hightemp | 高温告警 | INT |
| {  "cmd": " sdkdevicealarmset",  "method": "request",  "msgid": "0123456",  "sessionid": "262176",  "data": {  "smoke": 1,  "hightemp": 1,  }  } | | |

告警级别获取回复

Topic:mainserver/username\_包名\_UDID\_当前秒数/pullmsg

|  |  |  |
| --- | --- | --- |
| 参数定义 | 参数说明 | 取值范围 |
| statuscode | 状态码 | 200/401/500(Http状态码) |
| {  "cmd" : "sdkdevicealarmget ",  "method":"response",  "msgid":"0123456",  "data": {  "smoke": 1,  "hightemp": 1,  }  "statuscode" : 200  } | | |

## 智能告警数据请求

站内车牌区域数据请求

Topic:app/mainserver/pullmsg

|  |  |  |
| --- | --- | --- |
| 参数定义 | 参数说明 | 取值范围 |
| starttime | 开始时间 | 字符串，长度<128 |
| endtime | 结束时间 | 字符串，长度<128 |
| location | 当前省份 | 字符串，长度<128 |
| **{**  "cmd"**:** "getentranceplateanalysis"**,**  "method"**:** "response"**,**  "msgid"**:** "0123456"**,**  "sessionid"**:** "65536"**,**  "data"**:** **{**  "type"**:** 1,  "page"**:** 1,  "num"**:** 6  }  **}** | | |

站内加油趋势加油数据请求回复

Topic:mainserver/username\_包名\_UDID\_当前秒数/pullmsg

|  |  |  |
| --- | --- | --- |
| 参数定义 | 参数说明 | 取值范围 |
| statuscode | 状态码 | 200/401/500(Http状态码) |
| {  "cmd": "getintelligentalarm",  "method": "response",  "msgid": "0123456",  "data": {  "total": 13234,  "alarmlist": [  {  "type": 1,  "leave": 2,  "time": "2021-06-09 10:18:44",  "place": "chn\_5"  },  {  "type": 1,  "leave": 2,  "time": "2021-06-09 10:18:41",  "place": "chn\_5"  },  {  "type": 2,  "leave": 2,  "time": "2021-06-09 10:18:37",  "place": "chn\_5"  },  {  "type": 2,  "leave": 2,  "time": "2021-06-09 10:18:35",  "place": "chn\_5"  },  {  "type": 2,  "leave": 2,  "time": "2021-06-09 10:18:31",  "place": "chn\_5"  },  {  "type": 2,  "leave": 2,  "time": "2021-06-09 10:18:28",  "place": "chn\_5"  }  ]  },  "statuscode": 200  } | | |

## 告警占比数据获取

告警占比数据请求

Topic:app/mainserver/pullmsg

|  |  |  |
| --- | --- | --- |
| 参数定义 | 参数说明 | 取值范围 |
| starttime | 开始时间 | 字符串，长度<128 |
| endtime | 结束时间 | 字符串，长度<128 |
| **{**  "cmd"**:** " getalarmproportionanalysis"**,**  "method"**:** "response"**,**  "msgid"**:** "0123456"**,**  "sessionid"**:** "65536"**,**  "data"**:** **{**  "starttime": "2021-06-01",  "endtime"**:** "2021-06-30",  }  **}** | | |

告警占比数据请求回复

Topic:mainserver/username\_包名\_UDID\_当前秒数/pullmsg

|  |  |  |
| --- | --- | --- |
| 参数定义 | 参数说明 | 取值范围 |
| statuscode | 状态码 | 200/401/500(Http状态码) |
| {  "cmd": "getalarmproportionanalysis",  "method": "response",  "msgid": "0123456",  "data": {  "smokecount": 13228,  "hightemcount": 6  },  "statuscode": 200  } | | |

## 告警数据时段分析

告警占比数据请求

Topic:app/mainserver/pullmsg

|  |  |  |
| --- | --- | --- |
| 参数定义 | 参数说明 | 取值范围 |
| starttime | 开始时间 | 字符串，长度<128 |
| endtime | 结束时间 | 字符串，长度<128 |
| number | 当前省份 | 字符串，长度<128 |
| **{**  "cmd"**:** " getalarmperiodanalysis"**,**  "method"**:** "response"**,**  "msgid"**:** "0123456"**,**  "sessionid"**:** "65536"**,**  "data"**:** **{**  "starttime": "2021-06-01",  "endtime"**:** "2021-06-30",  " number "**: 30**  }  **}** | | |

告警占比数据请求回复

Topic:mainserver/username\_包名\_UDID\_当前秒数/pullmsg

|  |  |  |
| --- | --- | --- |
| 参数定义 | 参数说明 | 取值范围 |
| statuscode | 状态码 | 200/401/500(Http状态码) |
| {  "cmd": "getalarmperiodanalysis",  "method": "response",  "msgid": "0123456",  "data": {  "alarmlist": [  {  "smokecount": 13228,  "hightemcount": 6  },  {  "smokecount": 13228,  "hightemcount": 6  },  {  "smokecount": 13228,  "hightemcount": 6  },  {  "smokecount": 13226,  "hightemcount": 5  },  {  "smokecount": 12736,  "hightemcount": 4  },  {  "smokecount": 12736,  "hightemcount": 4  },  {  "smokecount": 12736,  "hightemcount": 4  },  {  "smokecount": 12736,  "hightemcount": 4  },  {  "smokecount": 6782,  "hightemcount": 4  },  {  "smokecount": 0,  "hightemcount": 0  },  {  "smokecount": 0,  "hightemcount": 0  },  {  "smokecount": 0,  "hightemcount": 0  },  {  "smokecount": 0,  "hightemcount": 0  },  {  "smokecount": 0,  "hightemcount": 0  },  {  "smokecount": 0,  "hightemcount": 0  },  {  "smokecount": 0,  "hightemcount": 0  },  {  "smokecount": 0,  "hightemcount": 0  },  {  "smokecount": 0,  "hightemcount": 0  },  {  "smokecount": 0,  "hightemcount": 0  },  {  "smokecount": 0,  "hightemcount": 0  },  {  "smokecount": 0,  "hightemcount": 0  },  {  "smokecount": 0,  "hightemcount": 0  },  {  "smokecount": 0,  "hightemcount": 0  },  {  "smokecount": 0,  "hightemcount": 0  },  {  "smokecount": 0,  "hightemcount": 0  },  {  "smokecount": 0,  "hightemcount": 0  },  {  "smokecount": 0,  "hightemcount": 0  },  {  "smokecount": 0,  "hightemcount": 0  },  {  "smokecount": 0,  "hightemcount": 0  },  {  "smokecount": 0,  "hightemcount": 0  }  ]  },  "statuscode": 200  } | | |

## 实时车俩数据统计推送

实时车俩数据统计推送

Topic:app/mainserver/pullmsg

|  |  |  |
| --- | --- | --- |
| 参数定义 | 参数说明 | 取值范围 |
| passingcount | 途经总数 | INT |
| incominfcount | 进站总数 | INT |
| {  "cmd": "getentrancevehiclessum",  "data": {  " passingcount ": 151,  " incominfcount ":0  } | | |

## 拐入率车辆列表获取

拐入率车辆列表数据获取请求

Topic:app/mainserver/pullmsg

|  |  |  |
| --- | --- | --- |
| 参数定义 | 参数说明 | 取值范围 |
| num | 获取列表数 | INT |
| **{**  "cmd"**:** " getentrancevehiclescurlist"**,**  "method"**:** "response"**,**  "msgid"**:** "0123456"**,**  "sessionid"**:** "65536"**,**  "data"**:** **{**  "num"**:** 10**,**  }  **}** | | |

拐入率车辆列表数据获取请求

Topic:mainserver/username\_包名\_UDID\_当前秒数/pullmsg

|  |  |  |
| --- | --- | --- |
| 参数定义 | 参数说明 | 取值范围 |
| statuscode | 状态码 | 200/401/500(Http状态码) |
|  | | |

## 拐入率数据推送

拐入率车辆数据推送

Topic:app/mainserver/pullmsg

|  |  |  |
| --- | --- | --- |
| 参数定义 | 参数说明 | 取值范围 |
| {  "cmd": "pushdeviceentrances",  "plateno": "无车牌",  "cartype": "其他",  "time": "2021-%02-06 25:15:36",  "refueno": 1  } | | |

## 告警推送

告警推送

Topic:app/mainserver/pullmsg

|  |  |  |
| --- | --- | --- |
| 参数定义 | 参数说明 | 取值范围 |
| {  "cmd": " pushalarmmessage",  "data"**:** **{**  "alarmtype"**:** 1**,**  "time"**:**"2021-06-25 16:12:00"**,**  "place"**:**"一号油站"  }  } | | |

## 临街车辆数据获取

临街车辆数据获取请求

Topic:app/mainserver/pullmsg

|  |  |  |
| --- | --- | --- |
| 参数定义 | 参数说明 | 取值范围 |
| starttime | 开始时间 | 字符串，长度<128 |
| endtime | 结束时间 | 字符串，长度<128 |
| **{**  "cmd"**:** "getfrontagevehiclessum"**,**  "method"**:** "response"**,**  "msgid"**:** "0123456"**,**  "sessionid"**:** "65536"**,**  "data"**:** **{**  "starttime"**:** "2021-06-17"**,**  "endtime"**:** "2021-06-18"**,**  }  **}** | | |

临街车辆数据请求回复

Topic:mainserver/username\_包名\_UDID\_当前秒数/pullmsg

|  |  |  |
| --- | --- | --- |
| 参数定义 | 参数说明 | 取值范围 |
| statuscode | 状态码 | 200/401/500(Http状态码) |
| {  "cmd": "getfrontagevehiclessum",  "method": "response",  "msgid": "0123456",  "data": {  "vancount": 0,  "buscount": 0,  "tructcount": 27,  "carcount": 13,  "othercount": 6,  "bluecount": 23,  "yellowcount": 21,  "greecount": 7,  "othercount": 6  },  "statuscode": 200  } | | |

## 进站率数据请求

临街车辆数据请求

Topic:app/mainserver/pullmsg

|  |  |  |
| --- | --- | --- |
| 参数定义 | 参数说明 | 取值范围 |
| starttime | 开始时间 | 字符串，长度<128 |
| endtime | 结束时间 | 字符串，长度<128 |
| **{**  "cmd"**:** "getentrancevehiclessum"**,**  "method"**:** "response"**,**  "msgid"**:** "0123456"**,**  "sessionid"**:** "65536"**,**  "data"**:** **{**  "starttime"**:** "2021-06-17"**,**  "endtime"**:** "2021-06-18"**,**  }  **}** | | |

临街车辆数据请求回复

Topic:mainserver/username\_包名\_UDID\_当前秒数/pullmsg

|  |  |  |
| --- | --- | --- |
| 参数定义 | 参数说明 | 取值范围 |
| statuscode | 状态码 | 200/401/500(Http状态码) |
| {  "cmd" : "getentrancevehiclessum ",  "method":"response",  "msgid":"0123456",  "statuscode" : 200，  "data":{  "passingcount": 100,  "incominfcount": 50  }  } | | |

## 站内车辆数据请求

站内车辆数据请求

Topic:app/mainserver/pullmsg

|  |  |  |
| --- | --- | --- |
| 参数定义 | 参数说明 | 取值范围 |
| page | 第几页 | INT |
| num | 每页请求的数量 | INT |
| vehicletype | 车辆类型 | INT |
| situationtype | 流失新增类型 | INT |
| fuzzystr | 关键字 | 字符串，长度<128 |
| starttime | 开始时间 | 字符串，长度<128 |
| endtime | 结束时间 | 字符串，长度<128 |
| **{**  "cmd"**:** "getentrancevehiclelist"**,**  "method"**:** "response"**,**  "msgid"**:** "0123456"**,**  "sessionid"**:** "65536"**,**  "data"**:** **{**  "page"**:** 1,  "num"**:** 10,  "situationtype"**:** 1,  "vehicletype"**:** 0,  "fuzzystr"**:**"京",  "starttime"**:** "2021-06-17"**,**  "endtime"**:** "2021-06-18"  }  **}** | | |

站内车辆数据请求回复

Topic:mainserver/username\_包名\_UDID\_当前秒数/pullmsg

|  |  |  |
| --- | --- | --- |
| 参数定义 | 参数说明 | 取值范围 |
| statuscode | 状态码 | 200/401/500(Http状态码) |
| {  "cmd": "getentrancevehiclelist",  "method": "response",  "msgid": "0123456",  "data": {  "total": 50,  "devicelist": [  {  "refueno": 1,  "plateno": "皖F7Q577",  "picpath": "http://10.67.0.99:80/picture/Streaming/tracks/303/?name=ch00003\_00000000656019023513600113480&size=113480",  "territory": "淮北市",  "plateclor": "蓝色",  "cartype": "轿车",  "time": "2021-06-10 14:47"  },  {  "refueno": 1,  "plateno": "冀A925YK",  "picpath": "http://10.67.0.99:80/picture/Streaming/tracks/303/?name=ch00003\_00000000656019062835200299512&size=299512",  "territory": "石家庄市",  "plateclor": "黄色",  "cartype": "货车",  "time": "2021-06-10 14:47"  },  {  "refueno": 1,  "plateno": "川A937E1",  "picpath": "http://10.67.0.99:80/picture/Streaming/tracks/303/?name=ch00003\_00000000656018987468800126723&size=126723",  "territory": "成都市",  "plateclor": "蓝色",  "cartype": "轿车",  "time": "2021-06-10 14:47"  },  {  "refueno": 1,  "plateno": "川A87FN7",  "picpath": "http://10.67.0.99:80/picture/Streaming/tracks/303/?name=ch00003\_00000000656018952652800120142&size=120142",  "territory": "成都市",  "plateclor": "蓝色",  "cartype": "其他",  "time": "2021-06-10 14:47"  },  {  "refueno": 1,  "plateno": "川AR9G42",  "picpath": "http://10.67.0.99:80/picture/Streaming/tracks/303/?name=ch00003\_00000000656018901043200252988&size=252988",  "territory": "成都市",  "plateclor": "蓝色",  "cartype": "货车",  "time": "2021-06-10 14:47"  },  {  "refueno": 1,  "plateno": "冀BC999P",  "picpath": "http://10.67.0.99:80/picture/Streaming/tracks/303/?name=ch00003\_00000000656018720000000114944&size=114944",  "territory": "唐山市",  "plateclor": "蓝色",  "cartype": "轿车",  "time": "2021-06-10 14:47"  },  {  "refueno": 1,  "plateno": "冀A908BB",  "picpath": "http://10.67.0.99:80/picture/Streaming/tracks/303/?name=ch00003\_00000000656018673715200224843&size=224843",  "territory": "石家庄市",  "plateclor": "黄色",  "cartype": "货车",  "time": "2021-06-10 14:47"  },  {  "refueno": 1,  "plateno": "冀A390EW",  "picpath": "http://10.67.0.99:80/picture/Streaming/tracks/303/?name=ch00003\_00000000656018634803200134508&size=134508",  "territory": "石家庄市",  "plateclor": "蓝色",  "cartype": "轿车",  "time": "2021-06-10 14:47"  },  {  "refueno": 1,  "plateno": "冀A908AF",  "picpath": "http://10.67.0.99:80/picture/Streaming/tracks/303/?name=ch00003\_00000000656018581145600270766&size=270766",  "territory": "石家庄市",  "plateclor": "黄色",  "cartype": "货车",  "time": "2021-06-10 14:47"  },  {  "refueno": 1,  "plateno": "川AU65N9",  "picpath": "http://10.67.0.99:80/picture/Streaming/tracks/303/?name=ch00003\_00000000656018542643200146944&size=146944",  "territory": "成都市",  "plateclor": "蓝色",  "cartype": "轿车",  "time": "2021-06-10 14:47"  }  ]  },  "statuscode": 200  } | | |

## 车辆历史记录数据请求

车辆历史记录数据请求

Topic:app/mainserver/pullmsg

|  |  |  |
| --- | --- | --- |
| 参数定义 | 参数说明 | 取值范围 |
| page | 页数 | INT |
| num | 每页请求的数量 | INT |
| location | 归属地 | 字符串，长度<128 |
| starttime | 开始时间 | 字符串，长度<128 |
| endtime | 结束时间 | 字符串，长度<128 |
| {  "clitopic": "CCSMP/123456/pullmsg",  "cmd": "getentrancehistorylist",  "method": "request",  "msgid": "0123456",  "sessionid": "262148",  "data": {  "page": 1,  "num": 10,  "location": "北京",  "plateno": "川A937ET"  }  } | | |

临街车辆数据请求回复

Topic:mainserver/username\_包名\_UDID\_当前秒数/pullmsg

|  |  |  |
| --- | --- | --- |
| 参数定义 | 参数说明 | 取值范围 |
| statuscode | 状态码 | 200/401/500(Http状态码) |
| {  "cmd": "getentrancehistorylist",  "method": "response",  "msgid": "0123456",  "data": {  "devicelist": [  {  "plateno": "川A937ET",  "territory": "省外",  "plateclor": "蓝色",  "cartype": "轿车",  "time": "2021-06-10 14:43"  }  ]  },  "statuscode": 200  } | | |

## 站内加油趋势数据请求

站内加油趋势数据请求

Topic:app/mainserver/pullmsg

|  |  |  |
| --- | --- | --- |
| 参数定义 | 参数说明 | 取值范围 |
| plateno | 车牌号码 | 字符串，长度<128 |
| time | 时间 | 字符串，长度<128 |
| **{**  "cmd"**:** "getentranceserviceanalysis"**,**  "method"**:** "response"**,**  "msgid"**:** "0123456"**,**  "sessionid"**:** "65536"**,**  "data"**:** **{**  "time"**:** "2021-06-18"  }  **}** | | |

站内加油趋势加油数据请求回复

Topic:mainserver/username\_包名\_UDID\_当前秒数/pullmsg

|  |  |  |
| --- | --- | --- |
| 参数定义 | 参数说明 | 取值范围 |
| statuscode | 状态码 | 200/401/500(Http状态码) |
| {  "cmd" : "getEntranceServiceAnalysis",  "method":"response",  "msgid":"0123456",  "statuscode" : 200，  "data":{  "devicecount": [  {  "count": 1,  },  {  "count": 3,  },  {  "count": 5,,  },  ] }  } | | |

## 站内车牌区域分析请求

站内车牌区域数据请求

Topic:app/mainserver/pullmsg

|  |  |  |
| --- | --- | --- |
| 参数定义 | 参数说明 | 取值范围 |
| starttime | 开始时间 | 字符串，长度<128 |
| endtime | 结束时间 | 字符串，长度<128 |
| location | 当前省份 | 字符串，长度<128 |
| **{**  "cmd"**:** "getentranceplateanalysis"**,**  "method"**:** "response"**,**  "msgid"**:** "0123456"**,**  "sessionid"**:** "65536"**,**  "data"**:** **{**  "starttime"**:** "2021-06-18",  "endtime"**:** "2021-06-19",  "location"**:** "湖南省"  }  **}** | | |

站内加油趋势加油数据请求回复

Topic:mainserver/username\_包名\_UDID\_当前秒数/pullmsg

|  |  |  |
| --- | --- | --- |
| 参数定义 | 参数说明 | 取值范围 |
| statuscode | 状态码 | 200/401/500(Http状态码) |
| {  "cmd": "getentranceplateanalysis",  "method": "response",  "msgid": "0123456",  "data": {  "province": 2,  "outprovince": 63  },  "statuscode": 200  } | | |

## 站内单台车辆加油趋势分析请求

单台车辆加油趋势数据请求

Topic:app/mainserver/pullmsg

|  |  |  |
| --- | --- | --- |
| 参数定义 | 参数说明 | 取值范围 |
| starttime | 开始时间 | 字符串，长度<128 |
| endtime | 结束时间 | 字符串，长度<128 |
| plateno | 车牌号 | 字符串，长度<128 |
| **{**  "cmd"**:** " getentrancehistorycount"**,**  "method"**:** "response"**,**  "msgid"**:** "0123456"**,**  "sessionid"**:** "65536"**,**  "data"**:** **{**  "starttime"**:** "2021-06-18",  "endtime"**:** "2021-06-19",  "plateno"**:** "川AAW777"  }  **}** | | |

站内加油趋势加油数据请求回复

Topic:mainserver/username\_包名\_UDID\_当前秒数/pullmsg

|  |  |  |
| --- | --- | --- |
| 参数定义 | 参数说明 | 取值范围 |
| statuscode | 状态码 | 200/401/500(Http状态码) |
| {  "cmd": "getentranceplateanalysis",  "method": "response",  "msgid": "0123456",  "data": {  "Province": 2,  "OutProvince": 63  },  "statuscode": 200  } | | |

## 站内加油（汽油，柴油）车辆数量分析

站内加油（汽油，柴油）车辆数量分析请求

Topic:app/mainserver/pullmsg

|  |  |  |
| --- | --- | --- |
| 参数定义 | 参数说明 | 取值范围 |
| starttime | 开始时间 | 字符串，长度<128 |
| endtime | 结束时间 | 字符串，长度<128 |
| **{**  "cmd"**:** " getrefuelingtypeanalysis"**,**  "method"**:** "response"**,**  "msgid"**:** "0123456"**,**  "sessionid"**:** "65536"**,**  "data"**:** **{**  "starttime"**:** "2021-06-18",  "endtime"**:** "2021-06-19",  }  **}** | | |

站内加油趋势加油数据请求回复

Topic:mainserver/username\_包名\_UDID\_当前秒数/pullmsg

|  |  |  |
| --- | --- | --- |
| 参数定义 | 参数说明 | 取值范围 |
| statuscode | 状态码 | 200/401/500(Http状态码) |
| {  "cmd": "getrefuelingtypeanalysis",  "method": "response",  "msgid": "0123456",  "data": {  "gasoline": 51,  "dieseloil": 102  },  "statuscode": 200  } | | |

## 出站车辆数据分析

出站车辆数量分析请求

Topic:app/mainserver/pullmsg

|  |  |  |
| --- | --- | --- |
| 参数定义 | 参数说明 | 取值范围 |
| starttime1 | 开始时间 | 字符串，长度<128 |
| endtime1 | 结束时间 | 字符串，长度<128 |
| starttime2 | 开始时间 | 字符串，长度<128 |
| endtime2 | 结束时间 | 字符串，长度<128 |
| number | 周期数 | INT |
| **{**  "cmd"**:** " getoutboundvehiclesanalysis"**,**  "method"**:** "response"**,**  "msgid"**:** "0123456"**,**  "sessionid"**:** "65536"**,**  "data"**:** **{**  "starttime1"**:** "2021-06-01",  "endtime1"**:** "2021-06-30",  "starttime2"**:** "2021-05-1",  "endtime2"**:** "2021-05-30",  "number":30  }  **}** | | |

站内加油趋势加油数据请求回复

Topic:mainserver/username\_包名\_UDID\_当前秒数/pullmsg

|  |  |  |
| --- | --- | --- |
| 参数定义 | 参数说明 | 取值范围 |
| statuscode | 状态码 | 200/401/500(Http状态码) |
| {  "cmd": "getoutboundvehiclesanalysis",  "method": "response",  "msgid": "0123456",  "data": {  "pass1total": 0,  "int1total": 0,  "pass2total": 0,  "int2total": 0,  "vehiclecount": [  {  "passingcount1": 0,  "incomingcount1": 0,  "passingcount2": 0,  "incomingcount2": 0  },  {  "passingcount1": 0,  "incomingcount1": 0,  "passingcount2": 0,  "incomingcount2": 0  },  {  "passingcount1": 0,  "incomingcount1": 0,  "passingcount2": 0,  "incomingcount2": 0  },  {  "passingcount1": 0,  "incomingcount1": 0,  "passingcount2": 0,  "incomingcount2": 0  },  {  "passingcount1": 0,  "incomingcount1": 0,  "passingcount2": 0,  "incomingcount2": 0  },  {  "passingcount1": 0,  "incomingcount1": 0,  "passingcount2": 0,  "incomingcount2": 0  },  {  "passingcount1": 0,  "incomingcount1": 0,  "passingcount2": 0,  "incomingcount2": 0  },  {  "passingcount1": 0,  "incomingcount1": 0,  "passingcount2": 0,  "incomingcount2": 0  },  {  "passingcount1": 0,  "incomingcount1": 0,  "passingcount2": 0,  "incomingcount2": 0  },  {  "passingcount1": 0,  "incomingcount1": 0,  "passingcount2": 0,  "incomingcount2": 0  },  {  "passingcount1": 0,  "incomingcount1": 0,  "passingcount2": 0,  "incomingcount2": 0  },  {  "passingcount1": 0,  "incomingcount1": 0,  "passingcount2": 0,  "incomingcount2": 0  },  {  "passingcount1": 0,  "incomingcount1": 0,  "passingcount2": 0,  "incomingcount2": 0  },  {  "passingcount1": 0,  "incomingcount1": 0,  "passingcount2": 0,  "incomingcount2": 0  },  {  "passingcount1": 0,  "incomingcount1": 0,  "passingcount2": 0,  "incomingcount2": 0  },  {  "passingcount1": 0,  "incomingcount1": 0,  "passingcount2": 0,  "incomingcount2": 0  },  {  "passingcount1": 0,  "incomingcount1": 0,  "passingcount2": 0,  "incomingcount2": 0  },  {  "passingcount1": 0,  "incomingcount1": 0,  "passingcount2": 0,  "incomingcount2": 0  },  {  "passingcount1": 0,  "incomingcount1": 0,  "passingcount2": 0,  "incomingcount2": 0  },  {  "passingcount1": 0,  "incomingcount1": 0,  "passingcount2": 0,  "incomingcount2": 0  },  {  "passingcount1": 0,  "incomingcount1": 0,  "passingcount2": 0,  "incomingcount2": 0  },  {  "passingcount1": 0,  "incomingcount1": 0,  "passingcount2": 0,  "incomingcount2": 0  },  {  "passingcount1": 0,  "incomingcount1": 0,  "passingcount2": 0,  "incomingcount2": 0  },  {  "passingcount1": 0,  "incomingcount1": 0,  "passingcount2": 0,  "incomingcount2": 0  }  ]  },  "statuscode": 200  }} | | |

## 异常车辆信息列表

异常车辆信息列表请求

Topic:app/mainserver/pullmsg

|  |  |  |
| --- | --- | --- |
| 参数定义 | 参数说明 | 取值范围 |
| num | 每页显示总数 | INT |
| page | 显示页数 | INT |
| starttime | 开始时间 | 字符串，长度<128 |
| endtime | 结束时间 | 字符串，长度<128 |
| **{**  "cmd"**:** " getabnormalvehiclelist "**,**  "method"**:** "response"**,**  "msgid"**:** "0123456"**,**  "sessionid"**:** "65536"**,**  "data"**:** **{**  "num"**:** 10,  "page"**:** 1,  "starttime"**:** "2021-06-18",  "endtime"**:** "2021-06-19"  }  **}** | | |

异常车辆信息列表请求请求回复

Topic:mainserver/username\_包名\_UDID\_当前秒数/pullmsg

|  |  |  |
| --- | --- | --- |
| 参数定义 | 参数说明 | 取值范围 |
| statuscode | 状态码 | 200/401/500(Http状态码) |
| {  "cmd": "getabnormalvehiclelist",  "method": "response",  "msgid": "0123456",  "data": {  "total": 1,  "vehiclelist": [  {  "staytime": 3600,  "plateno": "川A7X3G2",  "territory": "成都市",  "cartype": "其他",  "time": "2021-06-10 14:43:44"  }  ]  },  "statuscode": 200  } | | |

## 停留时间占比分析

停留时间占比分析请求

Topic:app/mainserver/pullmsg

|  |  |  |
| --- | --- | --- |
| 参数定义 | 参数说明 | 取值范围 |
| starttime | 开始时间 | 字符串，长度<128 |
| endtime | 结束时间 | 字符串，长度<128 |
| **{**  "cmd"**:** " getresidencetimeanalysis"**,**  "method"**:** "response"**,**  "msgid"**:** "0123456"**,**  "sessionid"**:** "65536"**,**  "data"**:** **{**  "starttime"**:** "2021-06-18",  "endtime"**:** "2021-06-19",  }  **}** | | |

站内加油趋势加油数据请求回复

Topic:mainserver/username\_包名\_UDID\_当前秒数/pullmsg

|  |  |  |
| --- | --- | --- |
| 参数定义 | 参数说明 | 取值范围 |
| statuscode | 状态码 | 200/401/500(Http状态码) |
| {  "cmd": "getresidencetimeanalysis",  "method": "response",  "msgid": "0123456",  "data": {  "count1": 63,  "count2": 1,  "count3": 1  },  "statuscode": 200  } | | |

## 加油效率分析

加油效率分析请求

Topic:app/mainserver/pullmsg

|  |  |  |
| --- | --- | --- |
| 参数定义 | 参数说明 | 取值范围 |
| number | 周期数 | INT |
| starttime | 开始时间 | 字符串，长度<128 |
| endtime | 结束时间 | 字符串，长度<128 |
| **{**  "cmd"**:** " getrefuelingefficiencyanalysis"**,**  "method"**:** "response"**,**  "msgid"**:** "0123456"**,**  "sessionid"**:** "65536"**,**  "data"**:** **{**  "number"**:** 30,  "starttime"**:** "2021-06-01",  "endtime"**:** "2021-06-30",  }  **}** | | |

站内加油趋势加油数据请求回复

Topic:mainserver/username\_包名\_UDID\_当前秒数/pullmsg

|  |  |  |
| --- | --- | --- |
| 参数定义 | 参数说明 | 取值范围 |
| statuscode | 状态码 | 200/401/500(Http状态码) |
| {  "cmd": "getrefuelingefficiencyanalysis",  "method": "response",  "msgid": "0123456",  "data": {  "vehiclecount": [  {  "total": 0,  "average": 0  },  {  "total": 0,  "average": 0  },  {  "total": 0,  "average": 0  },  {  "total": 0,  "average": 0  },  {  "total": 0,  "average": 0  },  {  "total": 0,  "average": 0  },  {  "total": 0,  "average": 0  },  {  "total": 0,  "average": 0  },  {  "total": 2,  "average": 1  },  {  "total": 50,  "average": 84  },  {  "total": 12,  "average": 0  },  {  "total": 0,  "average": 0  },  {  "total": 0,  "average": 0  },  {  "total": 0,  "average": 0  },  {  "total": 1,  "average": 60  },  {  "total": 0,  "average": 0  },  {  "total": 0,  "average": 0  },  {  "total": 0,  "average": 0  },  {  "total": 0,  "average": 0  },  {  "total": 0,  "average": 0  },  {  "total": 0,  "average": 0  },  {  "total": 0,  "average": 0  },  {  "total": 0,  "average": 0  },  {  "total": 0,  "average": 0  },  {  "total": 0,  "average": 0  },  {  "total": 0,  "average": 0  },  {  "total": 0,  "average": 0  },  {  "total": 0,  "average": 0  },  {  "total": 0,  "average": 0  },  {  "total": 0,  "average": 0  }  ]  },  "statuscode": 200  } | | |

## 车辆轨迹数据请求

车辆轨迹数据请求

Topic:app/mainserver/pullmsg

|  |  |  |
| --- | --- | --- |
| 参数定义 | 参数说明 | 取值范围 |
| page | 页数 | INT |
| num | 每页显示数目 | INT |
| starttime | 开始时间 | 字符串，长度<128 |
| endtime | 结束时间 | 字符串，长度<128 |
| **{**  "cmd"**:** " getvehicletrajectoryanalysis"**,**  "method"**:** "response"**,**  "msgid"**:** "0123456"**,**  "sessionid"**:** "65536"**,**  "data"**:** **{**  "page"**:** 1,  "num"**:** 10，  "starttime"**:** "2021-06-01",  "endtime"**:** "2021-06-30",  }  **}** | | |

车辆轨迹数据请求回复

Topic:mainserver/username\_包名\_UDID\_当前秒数/pullmsg

|  |  |  |
| --- | --- | --- |
| 参数定义 | 参数说明 | 取值范围 |
| statuscode | 状态码 | 200/401/500(Http状态码) |
| {  "cmd": "getvehicletrajectoryanalysis",  "method": "response",  "msgid": "0123456",  "data": {  "total": 65,  "vehiclelist": [  {    "tokenid ": " 20210702183714827 ",  "plateno": "川AAW777",  "picpath": "http://10.67.0.99:80/picture/Streaming/tracks/303/?name=ch00003\_00000000656014858291200131049&size=131049",  "territory": "成都市",  "plateclor": "蓝色",  "cartype": "其他"  "time": "2021-8-21 12:00:00"  },  {  "tokenid ": " 20210702183714827 ",  "plateno": "川AAW777",  "picpath": "http://10.67.0.99:80/picture/Streaming/tracks/303/?name=ch00003\_00000000746019372902400110496&size=110496",  "territory": "成都市",  "plateclor": "蓝色",  "cartype": "其他",  "time": "2021-8-21 12:00:00"  },  {  "tokenid ": " 20210702183714827 ",  "plateno": "冀DE527Y",  "picpath": "http://10.67.0.99:80/picture/Streaming/tracks/303/?name=ch00003\_00000000746019339315200103120&size=103120",  "territory": "邯郸市",  "plateclor": "蓝色",  "cartype": "其他",  "time": "2021-8-21 12:00:00"  },  {  "tokenid ": " 20210702183714827 ",  "plateno": "川AN12J3",  "picpath": "http://10.67.0.99:80/picture/Streaming/tracks/303/?name=ch00003\_00000000746019289344000256993&size=256993",  "territory": "成都市",  "plateclor": "蓝色",  "cartype": "其他",  "time": "2021-8-21 12:00:00"  },  {  "tokenid ": " 20210702183714827 ",  "plateno": "川AC59J1",  "picpath": "http://10.67.0.99:80/picture/Streaming/tracks/303/?name=ch00003\_00000000746001563904000200296&size=200296",  "territory": "成都市",  "plateclor": "黄色",  "cartype": "其他",  "time": "2021-8-21 12:00:00"  },  {  "tokenid ": " 20210702183714827 ",  "plateno": "川A6H3Q2",  "picpath": "http://10.67.0.99:80/picture/Streaming/tracks/303/?name=ch00003\_00000000804105982822400127640&size=127640",  "territory": "成都市",  "plateclor": "蓝色",  "cartype": "其他",  "time": "2021-8-21 12:00:00"  }  ]  },  "statuscode": 200  } | | |

## 车辆轨迹获取

车辆轨迹数据获取

Topic:app/mainserver/pullmsg

|  |  |  |
| --- | --- | --- |
| 参数定义 | 参数说明 | 取值范围 |
| plateno | 车牌号码 | 字符串，长度<128 |
| **{**  "cmd"**:** " getvehicletrajectoryroute"**,**  "method"**:** "response"**,**  "msgid"**:** "0123456"**,**  "sessionid"**:** "65536"**,**  "data"**:** **{**  "tokenid"**:** "20210701"**,**  }  **}** | | |

Topic:mainserver/username\_包名\_UDID\_当前秒数/pullmsg

|  |  |  |
| --- | --- | --- |
| 参数定义 | 参数说明 | 取值范围 |
| statuscode | 状态码 | 200/401/500(Http状态码) |
| {  "cmd": " getvehicletrajectoryroute",  "method": "response",  "msgid": "0123456",  "data": {  " arrivalstartdate ": "2021-6-30 8:00:00",  " arrivalenddate ": "2021-6-30 9:00:00",  " washstartdate": "2021-6-30 8:10:00",  " washenddate": "2021-6-30 8:20:00",  },  "statuscode": 200  } | | |

## 洗车占比数据请求

获取考勤打卡记录数据

Topic:app/mainserver/pullmsg

|  |  |  |
| --- | --- | --- |
| 参数定义 | 参数说明 | 取值范围 |
| starttime | 开始时间 | 字符串，长度<128 |
| endtime | 结束时间 | 字符串，长度<128 |
| **{**  "cmd"**:** " getproportionofcarwashing "**,**  "method"**:** "response"**,**  "msgid"**:** "0123456"**,**  "sessionid"**:** "65536"**,**  "data"**:** **{**  "starttime"**:** "2021-06-17"**,**  "endtime"**:** "2021-06-18"  }  **}** | | |

获取考勤打卡记录数据

Topic:mainserver/username\_包名\_UDID\_当前秒数/pullmsg

|  |  |  |
| --- | --- | --- |
| 参数定义 | 参数说明 | 取值范围 |
| statuscode | getproportionofvehiclebehavior状态码 | 200/401/500(Http状态码) |
| {  "cmd": " getproportionofcarwashing ",  "method": "response",  "msgid": "0123456",  "data": {  " washcount": 33,  " totalcount": 45,  " washwithoutaddnum": 45,  " addwithoutwashnum": 45,  " addandwashnum": 45,  " washandaddnum": 45,  },  "statuscode": 200  } | | |

## 车辆行为占比请求

获取考勤打卡记录数据

Topic:app/mainserver/pullmsg

|  |  |  |
| --- | --- | --- |
| 参数定义 | 参数说明 | 取值范围 |
| starttime | 开始时间 | 字符串，长度<128 |
| endtime | 结束时间 | 字符串，长度<128 |
| **{**  "cmd"**:** " getproportionofvehiclebehavior"**,**  "method"**:** "response"**,**  "msgid"**:** "0123456"**,**  "sessionid"**:** "65536"**,**  "data"**:** **{**  "starttime"**:** "2021-06-17"**,**  "endtime"**:** "2021-06-18"  }  **}** | | |

获取考勤打卡记录数据

Topic:mainserver/username\_包名\_UDID\_当前秒数/pullmsg

|  |  |  |
| --- | --- | --- |
| 参数定义 | 参数说明 | 取值范围 |
| statuscode | 状态码 | 200/401/500(Http状态码) |
| {  "cmd": " getproportionofvehiclebehavior ",  "method": "response",  "msgid": "0123456",  "data": {  " washcount ": 33,  " oilcount ": 45,  "count3": 28  },  "statuscode": 200  } | | |

## 获取考勤打卡记录

获取考勤打卡记录数据

Topic:app/mainserver/pullmsg

|  |  |  |
| --- | --- | --- |
| 参数定义 | 参数说明 | 取值范围 |
| page | 页数 | INT |
| num | 每页请求的数量 | INT |
| starttime | 开始时间 | 字符串，长度<128 |
| endtime | 结束时间 | 字符串，长度<128 |
| **{**  "cmd"**:** "getattendancelist"**,**  "method"**:** "response"**,**  "msgid"**:** "0123456"**,**  "sessionid"**:** "65536"**,**  "data"**:** **{**  "page"**:** 1,  "num"**:** 10,  "starttime"**:** "2021-06-17"**,**  "endtime"**:** "2021-06-18"  }  **}** | | |

获取考勤打卡记录数据

Topic:mainserver/username\_包名\_UDID\_当前秒数/pullmsg

|  |  |  |
| --- | --- | --- |
| 参数定义 | 参数说明 | 取值范围 |
| statuscode | 状态码 | 200/401/500(Http状态码) |
| {  "cmd" : "getattendancelist",  "method":"response",  "msgid":"0123456",  "statuscode" : 200，  "data":{  "attendancelist": [  {  "name": "xiaoming",  "usrid": "43252215555555555555",  "phonenum": "188888888888",  "time": "2021-5-20 16:40",  "snaptoken": "1212121212121",  "plateimagepath": "http://113.113.113.113",  "snapimagepath": "http://113.113.113.113"  },  {  "name": "xiaoming",  "usrid": "43252215555555555555",  "phonenum": "188888888888",  "time": "2021-5-20 16:40",  "snaptoken": "1212121212121",  "plateimagepath": "http://113.113.113.113",  "snapimagepath": "http://113.113.113.113"  },  {  "name": "xiaoming",  "usrid": "43252215555555555555",  "phonenum": "188888888888",  "time": "2021-5-20 16:40",  "snaptoken": "1212121212121",  "plateimagepath": "http://113.113.113.113",  "snapimagepath": "http://113.113.113.113"  },  ] }  } | | |

## 推送考勤打卡

推送考勤打卡数据

Topic:CCSMP/mainserver/pushmsg

|  |  |  |
| --- | --- | --- |
| 参数定义 | 参数说明 | 取值范围 |
| name | 员工名字 | 字符串 <64 |
| usrid | 身份证 | 字符串 <64 |
| phonenum | 手机号 | 字符串<12 |
| time | 抓拍时间 | 字符串<128 |
| snaptoken | 抓拍id | 字符串<128 |
| plateimagepath | 背景图 | 字符串<128 |
| snapimagepath | 人脸图 | 字符串<128 |
| {  "cmd" : "getattendancelist",  "method":"request",  "msgid":"0123456",  "statuscode" : 200，  "data":{    "name": "xiaoming",  "usrid": "43252215555555555555",  "phonenum": "188888888888",  "time": "2021-5-20 16:40",  "snaptoken": "12121212121",  "plateimagepath": "http://113.113.113.113",  "snapimagepath": "http://113.113.113.113"  } | | |

## 推送顾客进店次数

推送顾客进店数据

Topic:CCSMP/mainserver/pushmsg

|  |  |  |
| --- | --- | --- |
| 参数定义 | 参数说明 | 取值范围 |
| name | 员工名字 | 字符串 <64 |
| usrid | 身份证 | 字符串 <64 |
| phonenum | 手机号 | 字符串<12 |
| time | 抓拍时间 | 字符串<128 |
| snaptoken | 抓拍id | 字符串<128 |
| plateimagepath | 背景图 | 字符串<128 |
| snapimagepath | 人脸图 | 字符串<128 |
| storefrequency | 进店频率 | 整型 |
| {  "cmd" : "pushvisitors",  "method":"request",  "msgid":"0123456",  "data":{    "name": "xiaoming",  "usrid": "43252215555555555555",  "phonenum": "188888888888",  "time": "2021-5-20 16:40",  "snaptoken": "12121212121",  "plateimagepath": "http://113.113.113.113",  "snapimagepath": "http://113.113.113.113",  "storefrequency": 10  } | | |

## 推送客流量

推送客流量数据

Topic:CCSMP/mainserver/pushmsg

|  |  |  |
| --- | --- | --- |
| 参数定义 | 参数说明 | 取值范围 |
| leavenum | 离店人数 | 整型 |
| enternum | 进店人数 | 整型 |
| {  "cmd" : "pushvolumeofcommuters",  "method":"request",  "msgid":"0123456",  "data":{    "leavenum": 50,  "enternum": 50  } | | |

## 获取当日打卡人员考勤数据

获取当日打卡人员考勤数据

Topic:app/mainserver/pullmsg

|  |  |  |
| --- | --- | --- |
| 参数定义 | 参数说明 | 取值范围 |
| starttime | 开始时间 | 字符串，长度<128 |
| endtime | 结束时间 | 字符串，长度<128 |
| **{**  "cmd"**:** "getattendance"**,**  "method"**:** "response"**,**  "msgid"**:** "0123456"**,**  "sessionid"**:** "65536"**,**  "data"**:{**  "starttime"**:** "2021-06-17"**,**  "endtime"**:** "2021-06-18"  }  **}** | | |

获取考勤打卡记录数据

Topic:mainserver/username\_包名\_UDID\_当前秒数/pullmsg

|  |  |  |
| --- | --- | --- |
| 参数定义 | 参数说明 | 取值范围 |
| statuscode | 状态码 | 200/401/500(Http状态码) |
| {  "cmd" : "getattendance",  "method":"response",  "msgid":"0123456",  "statuscode" : 200，  "data":{  "attendancelist": [  {  "name": "xiaoming",  "usrid": "43252215555555555555",  "phonenum": "188888888888",  "time": "2021-5-20 16:40",  "snaptoken": "1212121212121",  "plateimagepath": "http://113.113.113.113",  "snapimagepath": "http://113.113.113.113"  },  {  "name": "xiaoming",  "usrid": "43252215555555555555",  "phonenum": "188888888888",  "time": "2021-5-20 16:40",  "snaptoken": "1212121212121",  "plateimagepath": "http://113.113.113.113",  "snapimagepath": "http://113.113.113.113"  },  {  "name": "xiaoming",  "usrid": "43252215555555555555",  "phonenum": "188888888888",  "time": "2021-5-20 16:40",  "snaptoken": "1212121212121",  "plateimagepath": "http://113.113.113.113",  "snapimagepath": "http://113.113.113.113"  },  ] }  } | | |

## 获取当日所有顾客进店数据

获取当日所有顾客进店数据

Topic:app/mainserver/pullmsg

|  |  |  |
| --- | --- | --- |
| 参数定义 | 参数说明 | 取值范围 |
| starttime | 开始时间 | 字符串，长度<128 |
| endtime | 结束时间 | 字符串，长度<128 |
| **{**  "cmd"**:** "getvisitors"**,**  "method"**:** "response"**,**  "msgid"**:** "0123456"**,**  "sessionid"**:** "65536"**,**  "data"**:{**  "starttime"**:** "2021-06-17"**,**  "endtime"**:** "2021-06-18"  }  **}** | | |

获取当日所有顾客进店数据

Topic:mainserver/username\_包名\_UDID\_当前秒数/pullmsg

|  |  |  |
| --- | --- | --- |
| 参数定义 | 参数说明 | 取值范围 |
| statuscode | 状态码 | 200/401/500(Http状态码) |
| {  "cmd" : "getvisitors",  "method":"response",  "msgid":"0123456",  "statuscode" : 200，  "data":{  "visitorslist": [  {  "storefrequency": 2,  "name": "xiaoming",  "time": "2021-5-20 16:40",  "snaptoken": "1212121212121",  "plateimagepath": "http://113.113.113.113",  "snapimagepath": "http://113.113.113.113"  },  {  "storefrequency": 2,  "name": "xiaoming",  "time": "2021-5-20 16:40",  "snaptoken": "1212121212121",  "plateimagepath": "http://113.113.113.113",  "snapimagepath": "http://113.113.113.113"  },  {  "storefrequency": 2,  "name": "xiaoming",  "time": "2021-5-20 16:40",  "snaptoken": "1212121212121",  "plateimagepath": "http://113.113.113.113",  "snapimagepath": "http://113.113.113.113"  },  ] }  } | | |